|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Site | Well length | riser | Installation Date | Notes |
| MM1W |  |  | April 2020 | Replacement for Odyssey recorder (3-4 WL). Logger installed during July 2020 trip? |
| MM2W | 60.5 in | 14.5 in | Dec 2019 | New well setup |
| MM3W | 10 ft | 8 in | April 2020 (new HOBO recorder to replace transducer) | Was originally a Dwyer setup, bad battery detected in April 2020 and replaced with HOBO WL. In downloads this is referred to as the lower well |
| MM4W | 66 in | 4 in | April 2020 | Replacement for Odyssey recorder (6-3 WL) |
| MM5W | 65 in | 3 in | April 2020 | Replacement for Odyssey recorder (9-3 WL) |
| MM6W | 76 in | 20 in | July 2020 | Replacement for Odyssey recorder (6-4 WL) |
| MM7W | 10 ft | 6.5 in | Sometime before July 2019 may have been July 2018 with the push probe | Hobo appears to have been here as of April 2019 |
| CM0W | 10 ft | 34 cm |  | Sometimes referred to as top/upper well in the notes |
| CM1W | 66 in | 8.5 in | Dec 2019 | Replacement for Odyssey recorder (C1-2 WL) |
| CM2W | 75.5 in | 23.5 in | Dec 2019 | Replacement for Odyssey recorder (C1-3 WL), this water level recorder was relocated in April 2020 to CM4W because the Dwyer setup at CM4W (lower well) went bad. For the time being, CM2W was replaced with an Odyssey |
| CM3W | 75.5 in | 23 in | Dec 2019 |  |
| CM4W | 10 ft | 9.3 cm |  | Sometimes referred to as the “lower control well” in notes |
| RC1W | 10 ft | 15 cm |  |  |
| RC2W | 1.5 m | 9 cm |  |  |
| RC3W | 10 ft | 42 cm |  |  |
| RC6W | 10 ft | 15 cm |  |  |